Definition: Potential difference is the amount of work done to move an electric charge from one point to another.

or

Definition: The definition of voltage is the electromotive force or the electrical potential difference between two points in a circuit expressed in volts.

Voltage is a scalar quantity. The SI unit of voltage is the volt, such that 1 volt = 1 joule/coulomb.

The easiest way to understand voltage is to use a water analogy. Using a hose as an example, think of voltage as the amount of pressure forcing water through a garden hose. The higher the pressure in the pipe the more water is forced through the pipe each second. The greater the voltage, the greater the flow of electrical current (that is, the quantity of charge carriers that pass a fixed point per unit of time Q=It) through a conducting or semiconducting medium for a given resistance to the flow.

One volt will drive one coulomb (6.24 × 1018) charge carriers, ( electrons), through a resistance of one ohm in one second.

Voltage can be direct or alternating. A direct voltage maintains the same polarity at all times. So charges always flow in one direction. In an alternating voltage, the polarity reverses direction periodically. The number of complete cycles per second is the frequency, which is measured in hertz (one cycle per second). An example of direct voltage is the potential difference between the terminals of a cell. Alternating voltage exists between the mains positive and negative.

Definition: Potential difference is the amount of work done to move an electric charge from one point to another.

or

Definition: The definition of voltage is the electromotive force or the electrical potential difference between two points in a circuit expressed in volts.

Voltage is a scalar quantity. The SI unit of voltage is the volt, such that 1 volt = 1 joule/coulomb.

The easiest way to understand voltage is to use a water analogy. Using a hose as an example, think of voltage as the amount of pressure forcing water through a garden hose. The higher the pressure in the pipe the more water is forced through the pipe each second. The greater the voltage, the greater the flow of electrical current (that is, the quantity of charge carriers that pass a fixed point per unit of time Q=It) through a conducting or semiconducting medium for a given resistance to the flow.

One volt will drive one coulomb (6.24 × 1018) charge carriers, ( electrons), through a resistance of one ohm in one second.

Voltage can be direct or alternating. A direct voltage maintains the same polarity at all times. So charges always flow in one direction. In an alternating voltage, the polarity reverses direction periodically. The number of complete cycles per second is the frequency, which is measured in hertz (one cycle per second). An example of direct voltage is the potential difference between the terminals of a cell. Alternating voltage exists between the mains positive and negative.

Definition: Potential difference is the amount of work done to move an electric charge from one point to another.

or

Definition: The definition of voltage is the electromotive force or the electrical potential difference between two points in a circuit expressed in volts.

Voltage is a scalar quantity. The SI unit of voltage is the volt, such that 1 volt = 1 joule/coulomb.

The easiest way to understand voltage is to use a water analogy. Using a hose as an example, think of voltage as the amount of pressure forcing water through a garden hose. The higher the pressure in the pipe the more water is forced through the pipe each second. The greater the voltage, the greater the flow of electrical current (that is, the quantity of charge carriers that pass a fixed point per unit of time Q=It) through a conducting or semiconducting medium for a given resistance to the flow.

One volt will drive one coulomb (6.24 × 1018) charge carriers, ( electrons), through a resistance of one ohm in one second.

Voltage can be direct or alternating. A direct voltage maintains the same polarity at all times. So charges always flow in one direction. In an alternating voltage, the polarity reverses direction periodically. The number of complete cycles per second is the frequency, which is measured in hertz (one cycle per second). An example of direct voltage is the potential difference between the terminals of a cell. Alternating voltage exists between the mains positive and negative.

Definition: Potential difference is the amount of work done to move an electric charge from one point to another.

or

Definition: The definition of voltage is the electromotive force or the electrical potential difference between two points in a circuit expressed in volts.

Voltage is a scalar quantity. The SI unit of voltage is the volt, such that 1 volt = 1 joule/coulomb.

The easiest way to understand voltage is to use a water analogy. Using a hose as an example, think of voltage as the amount of pressure forcing water through a garden hose. The higher the pressure in the pipe the more water is forced through the pipe each second. The greater the voltage, the greater the flow of electrical current (that is, the quantity of charge carriers that pass a fixed point per unit of time Q=It) through a conducting or semiconducting medium for a given resistance to the flow.

One volt will drive one coulomb (6.24 × 1018) charge carriers, ( electrons), through a resistance of one ohm in one second.

Voltage can be direct or alternating. A direct voltage maintains the same polarity at all times. So charges always flow in one direction. In an alternating voltage, the polarity reverses direction periodically. The number of complete cycles per second is the frequency, which is measured in hertz (one cycle per second). An example of direct voltage is the potential difference between the terminals of a cell. Alternating voltage exists between the mains positive and negative.